Site selection method

1. Place grid of 10ha cells over annual monitoring sites
2. Select one point per cell up to 64 points
3. Points that overlap grid lines not selected
4. Where two points were in a cell, the one furthest from selected points in adjacent cells was selected